**References**

. Becquerel A. E.. 1839 - Compt. Rend. Acad. Sci. 9 145.

. J.C. Hummelen, G. Yu, J. Gao, F. Wudl, A.J. Heeger - Polymer Photovoltaic Cell: Enhanced efficiency via a network of internal donor acceptor heterojunctions, Science, 270 (5243), 1789 (1995).

. P. Peumans and S.R. Forrest - Very-high-efficiency double heterostructure copper phthalocyanine/C60photovoltaic cells, ppl. Phys. Lett., 79 (1), 126 (2001); vgl. Erratum dazu: P. Peumans, S.R. Forrest, Appl. Phys. Lett., 80 (2), 338 (2002).

. W. Kern, D. Puotinen - Cleaning solutions based on hydrogen peroxide for use in silicon semiconductor technology. RCA Rev. 31:187-206, 1970. [RCA Laboratories, Princeton, and RCA Solid-State Division, Somerville, NJ]

. R. G. Gordon - Mater. Res. Soc. Symp. Proc. 426 (1996) 419; a similar expression was proposed by V. K. Jain and A. P. Kulshreshtha - Sol. Energy Mater. 4(1981) 151 without taking into account the reflection.

. B. Johnev, M. Vogel, K. Fostiropoulos, B. Mrusu, MC. Lux-Steiner, A. Weidinger - Monolayer passivation of the transparent electrode in organic solar cells, 2005 - Thin Solid Films, 488:270-273.

. Norrman K., Masen M.V., Gevorgyan S.A., Krebs F.C., 2010 - Degradation patterns in water and oxygen of an inverted polymer solar cell, Journal of the American Chemical Society. 132, 16883 16892.

. Berredjem Y., Bernède J.C., Ouro Djobo S., Cattin L., Morsli M., Boulmokh A., 2008 On the improvement of the efficiency of organic photovoltaic cells by the presence of an ultra-thin metal layer at the interface organic/ITO, Eur. Phys. J. Appl. Phys. 44, 223–228

. Boutaleb Y., Rehamnia R., Berredjem Y., Bernède J.C., 2015 - Nanostructured solar cells based on MoO3 film deposition. Revue des Energies Renouvelables Vol. 18 N°2 193 – 198

. Berredjem Y., Boulmokh A., Bensid N., Drici A., Gheid AEK., Bouras A., Bernède J.C., 2011 - Study of the insertion of a metal layer in an organic solar cell, J. Mater. Environ. Sci. Oujda.