**REFERENCES**

. Apkan U.G., Hameed B.H., 2009 - Parameters affecting the photocatalytic degradation of dyes using TiO2-based photocatalysts: A review, J. Hazard. Mater. 170 520–529.

. Malato S., Fernandez-Ibanez P., Maldonado M.I., Blanco J., Gernjak W., 2009 - Decontamination and disinfection of water by solar photocatalysis: Recent overview and trends. Catal. Today, 147, 1-59.

. Van de Giesen N., Van der Zaag P., Hoekstra A., 2012 - Recent advances in water resources management. Phys. Chem. Earth. Parts A/B/C 1, 47-48.

. Dijkstra M. F. J., Michorius A., Buwalda H., Panneman H. J., Winkelmann J. G. M., Beenackers A. A. C. M. Comparison of the efficiency of immobilized and suspended systems

. Shan A.Y., Ghazi T.I.M., Rashid S., 2010 - Immobilisation of titanium dioxide onto supporting materials in heterogenous photocatalysis: A review, Appl. Cat. A: General 389. 1–8.

. Shen C., Wang Y.J., Xu J.H., Luo G.S., 2012 - Facile synthesis and photocatalytic properties of TiO2 nanoparticles supported on porous glass beads, Chem. Eng. J. 209, 478– 485.

. Yildirim G., Bal S., Gulen M., Varilci A., Budak E., Akdogan M., 2012 - Substrate effect on microstructure and optical performance of sputter-deposited TiO2 thin films, Cryst. Res. Technol. 47, 195–201.

. Salatiel Wohlmuth da Silva., 2016 - TiO2 thick films supported on stainless steel foams and their photoactivity in the nonylphenol ethoxylate mineralization, Chem. Eng. J. 283, 1264–1272

. Yang L., Yu L.E., Ray M.B., 2008 - Degradation of paracetamol in aqueous solutions by TiO2 photocatalysis, Water Res. 42, 3480–3488.

. Bianchi C.L., Pirola C., Selli E., Biella S., 2012 - Photocatalytic NOx abatement: The role of the material supporting the TiO2 active layer, J. Hazard Mater. 211–212, 203–207.

. Tusnelda E.D., Fritz H.F., 2004 - Development of easy and reproducible immobilization techniques using TiO2 for photocatalytic degradation of aquatic pollutants, Actahydrochim. hydrobiol. 32(3), 201–213.

. Chunhong Ma., 2015 - Study on photocatalytic activity of Er3+:YAlO3/TiO2 composite films supported on electrically conductive glass (FTO) in visible-light photocatalytic degradation of organic dye, Sep. Purif. Technol., 148, 76–84.