**References**

. Sze S.M., 1994 - Semiconductor sensors. Ed. J. Wiley and Sons, New York, USA.

. Schmitz V., Schelten J., 2004 - Double electron drift device as a magnetic field sensor. Microelectronic engineering, vol. 73, no. 1 : 519-523.

. Roumenin Ch., 1990 - Bipolar magnetotransistor sensors , Sensors and actuators A, vol. 24, no. 2: 83-105.

. Schmitz V., Schelten J., 2003 - Split-electrode drift device as magnetic-field sensor, Sensors and actuators A, vol. 109, no. 1-3: 25-33

. Von Kluge J.W.A., 2001 - Analysis of split-current magnetic field sensitive resistors, Sensors and actuators A, vol. 93, no. 2: 103-108.

. Demierre M., Pesenti S., Frounchi J., Besse P.A., Popovic R.S., 2002 - Reference magnetic actuator for self-calibration of a very small Hall sensor array, Sensors and actuators A, vol. 97-98: 39-46.

. Roumenin Ch., Nikolov D., Ivanov A., 2004 - 3-D silicon vector sensor based on a novel parallel-field Hall microdevice, Sensors and actuators A, vol. 110, no. 1-3: 219-227.

. Wolffenbuttel R.F., 1996 - Silicon sensors and circuits, Ed. Chapman and Hall, London.

. Kireev P., 1975 - La physique des semiconducteurs, Ed. Mir, Moscou.

. Mathieu H., 1987 - Physique des semiconducteurs et des composants électroniques, Ed. Masson, Paris.