**References**

. Alfegi E.M.A., 2009 - Mathematical model of double pass photovoltaic thermal air collector with fins. American Journal of Environmental Sciences 5: 592-598.

. Naphon P., 2005 - Effect of porous media on the performance of the double-pass flat plate solar air heater. International Communications in Heat and Mass Transfer 32: 140–150.

. Sopian K., 2009 - Evaluation of thermal efficiency of double-pass solar collector with porous-nonporous media. Renewable Energy 34: 640–645.

. Ramadan M.R.I., 2007 - Thermal performance of a packed bed double-pass solar air heater, Energy 32: 1524–1535.

. Kumar P., 2012 - Effect of differential mass flow rate on the thermal performance of double duct packed bed solar air heaters. International Conference on Renewable Energies and Power Quality (ICREPQ’12), Santiago de Compostela (Spain), 28th to 30th March

. Ho C.D., Chen T.C. 2006 - The recycle effect on the collector efficiency improvement of double-pass sheet-and-tube solar water heaters with external recycle. Renewable Energy 31: 953–970.

. Ho C.D., Chen T.C., 2008 - Collector efficiency improvement of recyclic doublepass sheet-and-tube solar water heaters with internal fins attached. Renewable Energy 33: 655–664.

. Ramani B.M., Gupta A., Kumar R., 2010 - Performance of a double pass solar air collector. Solar Energy 84: 1929–1937

. Korti A. N., 2015 - Numerical 3D heat flow simulations on double pass solar collector with and without porous media. Journal of Thermal Engineering 1: 10-23.